For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. The hood must be in the open position for the removal of the plenum water deflector.
2. Remove both windshield wiper arms. Refer to Windshield Wiper Arm Replacement.

1 | Air Inlet Grille Panel Retainer (Qty: 4)
2 | Air Inlet Grille Panel

#### Procedure

1. Pull the plenum water deflector up at the windshield edge.
2. Pull the plenum water deflector over both windshield wiper arm pivot shafts.
3. Disengage the hose at the windshield washer nozzle connection.