For 1990-2009 cars

## Starter Replacement 2.0L Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the engine shield. Refer to Engine Shield Replacement.

1 | Battery Cable Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the cable from the starter motor.

Tighten
8 N·m (71 lb in)

2 | Starter Motor Fastener (Qty: 3) Tighten 22 N·m (16 lb in)
3 | Starter Motor

## Starter Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Battery Cable Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Starter Motor Retainer
3 | Starter Motor Fastener (Qty: 2) Tighten X N·m (X lb in)
4 | Starter Motor

#### Procedure

Disconnect any electrical connectors.

## Starter Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Starter Motor Wiring Harness (Qty: 3)
2 | Starter Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip

• | Remove the upper starter fastening bolt before lifting the vehicle.

• | Disconnect the crankshaft position sensor electrical connector. Remove the connector from the bracket.

Tighten
25 N·m (18 lb ft)

3 | Starter Motor

## Starter Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove secondary air injection pump. Refer to LINK.

1 | Starter Motor Wiring Harness Fastener

#### Procedure

Disconnect the electrical connector of the knock sensor.

Caution: Refer to Fastener Caution in the Preface section.

Tighten
X N·m (X lb ft)

2 | Starter Motor Wiring Harness Fastener Tighten X N·m (X lb ft)
3 | Starter Fastener (Qty: 2) Tighten 47 N·m (34 lb ft)
4 | Starter Motor