For 1990-2009 cars

#### Special Tools

(GLOBAL NR REQUIRED) Valve Spring Tester

### Inspection Procedure

1. Clean the valve springs in solvent.

Warning: Wear safety glasses when using compressed air, as flying dirt particles may cause eye injury.

2. Dry the valve springs with compressed air.
3. Inspect the valve springs for broken coils or coil ends.

### Measurement Procedure

1. Measure the valve spring tension using the J 22738-B (GLOBAL NR REQUIRED) tester . Refer to Engine Mechanical Specifications.
2. If low valve spring load is found, replace the valve springs. DO NOT use shims to increase spring load. The use of shims can cause the valve spring to bottom out before the camshaft lobe is at peak lift.