For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove engine appearance cover replacement. Refer to LINK.

1 | Fuel Feed Pipe retainer (Qty: 4) Caution: Do not allow the fuel pressure to exceed the specified value because damage to the fuel pressure regulator or the fuel pressure gage may result.
2 | Fuel Feed Pipe

#### Procedure

Open the both retainer with a small screwdriver