For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the engine cover. Refer to Link.

1 | Camshaft Position Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 15 N·m (11 lb ft)
2 | Camshaft Position Sensor

#### Procedure

Disconnect the electrical connector.