For 1990-2009 cars

## Rear Brake Rotor Replacement J60

Callout | Component Name
--- | ---
Warning: Refer to Brake Dust Warning in the Preface section.

#### Preliminary Procedures

Remove the brake caliper mounting bracket. Refer to Rear Brake Caliper Bracket Replacement.

1 | Rotor Retention Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (88 lb in)
2 | Brake Rotor

#### Procedure

1. If removing the rotor to service the wheel bearing/hub, use a rotory steel wire brush. Clean the contact area of the rotor to the wheel bearing/hub.
2. If servicing the rotor, use a rotory steel wire brush. Clean the contact area of the wheel bearing/hub.

## Rear Brake Rotor Replacement J61, J62

Callout | Component Name
--- | ---
Warning: Refer to Brake Dust Warning in the Preface section.

#### Preliminary Procedures

Remove the brake caliper mounting bracket. Refer to Rear Brake Caliper Bracket Replacement.

1 | Rotor Retention Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Brake Rotor

#### Procedure

1. If removing the rotor to service the wheel bearing/hub, use a rotory steel wire brush. Clean the contact area of the rotor to the wheel bearing/hub.
2. If servicing the rotor, use a rotory steel wire brush. Clean the contact area of the wheel bearing/hub.