For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove rear seat back. Refer to Link.
2. Remove rear seat cushion. Refer to Rear Seat Head Restraint Replacement.

1 | Rear Seat Back Cushion Hinge Control Fastener ( Qty: 3 )
2 | Rear Seat Back Cushion Hinge

#### Procedure

1. Pull the left and right rear seat backrest apart.
2. Detach the rear seat back cushion hinge from the guide pin.