For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Windshield Washer Solvent Level Sensor

#### Procedure

1. Disconnect the windshield washer solvent level sensor electrical connector.
2. Drain the windshield washer solvent container into a clean suitable container.
3. Pull the windshield washer solvent level sensor out of the windshield washer solvent container.
4. Using a small flat-bladed tool, remove the windshield washer solvent level sensor seal from the windshield washer solvent container and inspect the seal, replace if damaged.