For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the Front Floor Console. Refer to Front Floor Console Replacement.
2. Remove the Front Floor Console Rear Air Duct. Refer to Front Floor Console Rear Air Duct Replacement.
3. Release the Transmission Shift Lever Cable from the Shift Control Lever. Refer to Shift Control Lever Replacement.
4. Remove the Battery Tray. Refer to Battery Tray Replacement.

1 | Manual Transmission Shift Lever Cable (Qty: 2)

#### Procedure

1. Detach 2 gearshift cable from shift linkage lever.
2. Remove 2 shift cable from counterhold.
3. Remove 2 shift cables.
4. On Installation ensure that both cables are correctly routed.
5. On installation before clamping the cables at both ends, adjust shift cables. Refer to Manual Transmission Shift Lever Cable Adjustment.