For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper in order to access the locking tabs on the radiator upper grille assembly. Refer to Front Bumper Fascia Replacement
2. Remove the front bumper fascia energy upper absorber. Refer to Front Bumper Fascia Energy Upper Absorber Replacement

1 | Radiator Upper Grille Tip Release the twenty seven front bumper tabs from the radiator upper grille and remove from the inside front bumper.