For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Instrument Panel Outer Trim Cover Retainer (Qty: 2) Tip Use a flat-bladed plastic trim tool to aid in the removal of the outer trim cover assembly.
2 | Instrument Panel Outer Trim Cover

#### Procedure

1. Disconnect the electrical connection.
2. When replacing the instrument panel outer trim cover, transfer the inflatable restraint disable switch.