For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the Front Side Door Outside Rearview Mirror Filler. Refer to LINK.

1 | Front Side Door Pull Handle Cover
2 | Front Side Door Handle Cover Tip Pull handle back to remove cap. Use suitable tool to unsnap.
3 | Front Side Door Inside Handle Fastener
4 | Front Side Door Pull Handle Fastener (Qty: 2)
5 | Front Side Door Trim Panel Retainer (Qty: 8)
6 | Front Side Door Trim Panel

#### Procedure

1. Use a KM-569-A plug lifter to aid in the removal of the door trim panel.
2. Pull upwards on the door lock retainer cable to disengage.
3. Disconnect electrical connector.

#### Special Tools

KM-569-A Plug Lifter

For equivalent regional tools, refer to Special Tools