For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the plenum water deflector. Refer to Plenum Water Deflector Replacement.
2. Remove the windshield wiper system module. Refer to Windshield Wiper System Module Replacement.

1 | Windshield Wiper Motor Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 4.5 N·m (40 lb in)
2 | Wiper Motor Crank Arm Fastener
3 | Windshield Wiper Motor Tip Use the BO-6626 puller to separate the transmission arm from the wiper motor crank arm.

#### Special Tools

BO-6626 Wiper Arm Puller

For equivalent regional tools, refer to Special Tools.