For 1990-2009 cars

## Air Inlet Valve Actuator Replacement Left Hand Drive and CJ2

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel (I/P) lower extension side trim panel. Refer to Instrument Panel Lower Extension Side Trim Panel Replacement.
3. Remove the temperature valve actuator - right side. Refer to Temperature Valve Actuator Replacement - Right Side.
4. Remove the heater and blower and air conditioning control module. Refer to Heater and Blower and Air Conditioning Control Module Replacement.
5. Remove the recirculation actuator. Refer to Recirculation Actuator Replacement.

1 | Air Inlet Valve Actuator Fastener (Qty: 2)

#### Procedure

Disconnect the air inlet valve actuator electrical connector.

2 | Air Inlet Valve Actuator Tip Actuator is self-calibrating when connecting the battery.

## Air Inlet Valve Actuator Replacement Left Hand Drive

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel (I/P) lower extension side trim panel. Refer to Instrument Panel Lower Extension Side Trim Panel Replacement.

1 | Air Inlet Valve Actuator Fastener (Qty: 3)

#### Procedure

Disconnect the air inlet valve actuator electrical connector.

Tip
Use an offset box wrench for the screw behind above.

2 | Air Inlet Valve Actuator Tip Actuator is self-calibrating when connecting the battery.