For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front side door water deflector. Refer to Front Side Door Water Deflector Replacement.
2. Remove the front side door outside handle. Refer to Front Side Door Outside Handle Replacement.

1 | Front Side Door Outside Handle Bracket Fastener
2 | Front Side Door Outside Handle Bracket

#### Procedure

1. Release front side door outside handle rod mechanism at shift linkage lever - clip.
2. Release the front side door lock cylinder rod from the door lock.
3. Transfer components as necessary.