For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Release the radiator surge tank engine hose. Refer to Radiator Surge Tank Engine Hose Replacement.
3. Release the radiator outlet hose. Refer to Radiator Outlet Hose Replacement.

1 | Engine Oil Cooler Core Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb in)
2 | Engine Oil Cooler Core