For 1990-2009 cars

1. Install the NEW turbocharger exhaust pipe gasket (1).
2. Install the exhaust turbocharger inlet pipe bank 1 (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the 5 NEW turbocharger exhaust pipe nuts (3) and tighten to 30 N·m (22 lb ft).
4. Install the exhaust heat shield bank 1 (2).
5. Install the 5 exhaust heat shield bolts (1) and tighten to 10 N·m (89 lb in).