For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the battery tray. Refer to Battery Tray Replacement.
2. Ensure that the shift control range select lever is in the park (P) position.
3. Using the TBD remover , disconnect the shift control cable from the transaxle range switch lever.
4. Depress the shift control cable retainer clip tabs and remove the shift control cable from the shift control cable bracket.

#### Special Tools

TBD Facia Retainer Remover

For equivalent regional tools refer to Special Tools.

1 | Automatic Transmission Range Selector Lever Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 15 N·m(11 lb ft)
2 | Automatic Transmission Range Selector Lever Washer
3 | Automatic Transmission Range Selector Lever