For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Inflator Module Handling and Storage Warning in the Preface section. Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedure

Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.

1 | Inflatable Restraint Steering Wheel Module Retainer (Qty: 2)

#### Procedures

1. Lower the steering column and move to the maximum rear end position.
2. Insert a small bended screw driver, or equivalent tool, through the access openings on the rear left and right side of the steering wheel.
3. Push the spring fastener inward to release the steering wheel inflator from the steering wheel.

2 | Inflatable Restraint Steering Wheel Module Assembly

#### Procedures

1. Disconnect the electrical connectors.
2. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping.