For 1990-2009 cars

## Knock Sensor Replacement Right Side

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the oil level indicator and tube.

1 | Knock Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Knock Sensor

#### Procedure

Disconnect the electrical connector.

## Knock Sensor Replacement Left Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Knock Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Knock Sensor

#### Procedure

Disconnect the electrial connector.