For 1990-2009 cars

### Removal Procedure

1. Remove cover cap (1) from the rear side door.

Using a small flat-bladed tool, release the cover cap from the rear side door.

2. Remove the rear side door outside handle from the rear side door.

• | Pull the rear side door outside handle (2) outwards and hold.

• | Turn fastener (1) to the left and to the mechanical stop.

| Note: Rear side door outside handle (2) must now be secured in pulled position.

3. Remove fixed rear handle part (1).
4. Pull the rear side door outside handle (1) to the rear and remove.

### Installation Procedure

1. Install the rear side door outside handle.

• | Install the rear side door outside handle.

• | Insert fixed rear handle part.

• | Turn fastener to the right and to the mechanical stop.

| Note: Hold the rear side door outside handle taut while screwing and lightly counterhold fixed handle part.

2. Install the cover cap into the rear side door.