For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the windshield washer solvent container filler tube. Refer to Windshield Washer Solvent Container Filler Tube Replacement.
2. Release the front wheelhouse front liner, if necessary. Refer to Front Wheelhouse Front Liner Replacement.

1 | Windshield Washer Solvent Container Fastener (Qty: 3)
2 | Windshield Washer Solvent Container

#### Procedure

1. Disconnect the hose from the windshield washer pump.
2. Disconnect the hose from the headlamp washer pump.
3. Disconnect the windshield washer solvent level indicator electrical connector.
4. Release the hoses and electrical wiring from the windshield washer solvent container.