For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. SIR disabling and enabling. Refer to SIR Disabling and Enabling.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
3. SIR seatbelt pretensioner handling warning. Refer to SIR Seatbelt Pretensioner Handling Warning.
4. Remove front seat adjuster track finish cover.Refer to Front Seat Adjuster Track Finish Cover Replacement.
5. Remove driver or passenger seat adjuster finish cover. Refer to Driver or Passenger Seat Adjuster Finish Cover Replacement.

1 | Front Seat Belt Tensioner Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Disconnect wiring harness connector of seat belt tensioner.
2. Cut cable strap at seat belt tensioner and detach wiring harness.
3. Unscrew fastener.
4. Remove seat belt tensioner from seat frame.

Tighten
45 N·m (33 lb ft)

2 | Front Seat Belt Tensioner