For 1990-2009 cars

## Rear Seat Back Cushion Pad Replacement Left Side

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear back seat-left side. Refer to LINK.
3. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement.
4. Remove the rear seat center head restraint. Refer to Rear Seat Center Head Restraint Installation.
5. Remove the rear seat head restraint guides. Refer to Rear Seat Head Restraint Guide Replacement.
6. Remove the rear seat back cushion latch release knob bezel. Refer to Rear Seat Back Cushion Latch Release Knob Bezel Replacement.
7. Remove the rear seat armrest frame bracket. Refer to LINK.
8. Remove the rear compartment access door. Refer to LINK.
9. Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement - Left Side.

1 | Rear Seat Back Cushion Cover

#### Procedure

Remove the hog rings that secure the rear seat back cushion cover to the pad.

2 | Rear Seat Cushion Pad