For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the lower control arm. Refer to Lower Control Arm Replacement.

1 | Front Lower Control Arm Bushing Fastener

#### Procedure

The bushing need to be in a certain position when the torque is tightened. For tightening, refer to Lower Control Arm Replacement.

2 | Front Lower Control Arm Bushing