For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel upper center trim panel. Refer to Instrument Panel Upper Center Trim Panel Replacement.

1 | Driver Information Display

#### Procedure

1. Remove the driver information display from the instrument panel upper center trim panel.
2. Disconnect the electrical connections.
3. For programming and set up information refer to Control Module References.