For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the quarter inner trim finish panel. Refer to Quarter Inner Trim Finish Panel Replacement.

1 | Radio Speaker Amplifier Bracket Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the fuel pump flow control module electrical connector.

Tighten
9 N·m (8 lb in)

2 | Fuel Pump Flow Control Module Fastener

#### Procedure

Separate the fuel pump flow control module from the radio speaker amplifier bracket.

Tighten
6.5 N·m (58 lb in)

3 | Radio Speaker Amplifier Bracket