For 1990-2009 cars

## Generator Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the secondary air injection inlet pipe. Refer to Secondary Air Injection Pump Replacement.
2. Remove the charge air cooler outlet hose. Refer to Charge Air Cooler Outlet Hose Replacement.
3. Drain the cooling system. Refer to Cooling System Draining and Filling.
4. Remove the drive belt from the pulley belt idler. Refer to Drive Belt Replacement.
5. Remove the front bumper fascia center support bracket. Refer to Front Bumper Fascia Center Support Bracket Replacement.
6. Remove the radiator upper bracket. Refer to Radiator Replacement.

1 | Generator Pulley Belt Idler Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 15 N·m (11 lb ft)
2 | Generator Pulley Belt Idler
3 | Generator Wiring Harness Connector

#### Procedure

1. Disconnect the electrical connector.
2. Remove the wiring harness fastener.

4 | Generator Fastener (Qty: 2) Tighten 35 N·m (25 lb ft)
5 | Generator

#### Procedure

1. Remove the charge air cooler outlet duct bracket.
2. Remove the engine oil cooler hose from engine oil cooler pipe.

## Generator Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the drive belt. Refer to Drive Belt Replacement.
3. Remove the power steering pump. Refer to Power Steering Pump Replacement.

1 | Generator Wiring Harness Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten
15 N·m (11 lb ft)

2 | Generator Fastener (Qty: 3) Tighten 23 N·m (17 lb ft)
3 | Generator

## Generator Replacement LDE/A16XER, 2HO/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the drive belt. Refer to Drive Belt Replacement.

1 | Generator Wiring Harness Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten

• | M6 - 8 N·m (71 lb in)

• | M8 - 15 N·m (11 lb ft)

2 | Generator Fastener (Qty: 2) Tighten 35 N·m (25 lb ft)
3 | Generator