For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the propeller shaft. Refer to Propeller Shaft Replacement.

1 | Dust Shield

#### Procedure

Install the dust shield using DT-49095 installer .

#### Special Tools

DT-49095 Seal Installer

2 | Rear Output Shaft Seal

#### Procedure

Install the shaft seal using DT-49097 installer and DT-49061 cone .

#### Special Tools

• | DT-49061 Entry Cone

• | DT-49097 Seal Installer