For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Brake Dust Warning in the Preface section. Caution: Support the brake caliper with heavy mechanic wire, or equivalent, whenever it is separated from its mount and the hydraulic flexible brake hose is still connected. Failure to support the caliper in this manner will cause the flexible brake hose to bear the weight of the caliper, which may cause damage to the brake hose and in turn may cause a brake fluid leak.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Unbolt and support the brake calliper with heavy mechanic wire or equivalent, without disconnecting the hydraulic brake flexible house.

1 | Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the bracket bolts from the steering gear knuckle.

Tighten
150 N·m(110 lb ft) +45 degrees +15 degrees

2 | Front Brake Caliper Bracket