For 1990-2009 cars

## Exhaust Manifold Heat Shield Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine cover. Refer to Engine Cover Replacement.

1 | Exhaust Manifold Heat Shield Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Exhaust Manifold Heat Shield

## Exhaust Manifold Heat Shield Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the Turbocharger Heat Shield. Refer to LINK.

1 | Exhaust Manifold Heat Shield Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Exhaust Manifold Heat Shield