For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Place the rear door window in the full down position.
2. Remove the rear side door window outer sealing strip. Refer to Rear Side Door Window Outer Sealing Strip Replacement.

1 | Rear Side Door Window Frame Front Cover Fastener (Qty: 3)

#### Procedure

Pull the rear side door window weatherstrip from the applique to expose the fasteners.

2 | Rear Side Door Window Frame Front Cover