For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left front wheel. Refer to Tire and Wheel Removal and Installation.
2. Remove the left lower control arm. Refer to LINK.
3. Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Wheel Drive Shaft Oil Seal

#### Procedure

1. Use the KM-557-A puller set to aid in the removal of the front wheel drive shaft oil seal.
2. Use the KM-519 installer drift to install the front wheel drive shaft oil seal.

#### Special Tools

• | KM-577-A Puller Set

• | KM-519 Installer Drift