For 1990-2009 cars

## Front Seat Tilt Adjuster Actuator Replacement Driver/Passenger Seat 6-Way Hybrid

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove driver or passenger seat. Refer to Driver or Passenger Seat Replacement
2. Remove driver or passenger seat adjuster finish cover. Refer to Driver or Passenger Seat Adjuster Finish Cover Replacement

1 | Front Seat Tilt Adjuster Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove the front seat out of vehicle.
2. Remove the driver or passenger seat adjuster finish cover.
3. Remove the tilt adjuster lever.

Tighten
19.5 N·m (15 lb ft)

2 | Front Seat Tilt Adjuster

## Front Seat Tilt Adjuster Actuator Replacement Driver/Passenger Seat 8-Way Power

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the driver or passenger seat. Refer to Driver or Passenger Seat Replacement.

1 | Securing Clip
2 | Roll Pin Tip Use a hammer and small round tool to tap the roll pin out.
3 | Front Seat Tilt Adjuster Actuator

#### Procedure

Disconnect the electrical connector.