For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement - Left Side.
2. Remove the driver side instrument panel molding - driver side. Refer to Instrument Panel Molding Replacement - Driver Side.

1 | Instrument Panel Lower Trim Panel Assembly Fastener (Qty: 5)
2 | Instrument Panel Lower Trim Panel Assembly

#### Procedure

1. Grasp the instrument panel lower trim panel assembly and pull rearward disengaging the retainer securing it to the instrument panel.
2. Release the diagnostic link.

3 | Instrument Panel Outer Compartment

#### Procedure

When replacing the instrument panel lower trim panel, transfer instrument panel outer compartment.