For 1990-2009 cars

#### Special Tools

EN-43653 Flywheel Holding Tool

For equivalent regional tools, refer to Special Tools.

#### Engine Flywheel with Manual Transmission

1. Install EN-43653 flywheel holding tool (1) in the starter assembly location, engaging the flywheel, in order to prevent crankshaft rotation.
2. Remove the flywheel attaching bolts.
3. Remove the flywheel (1).
4. Remove the pilot bearing.
5. Remove EN-43653 flywheel holding tool .

#### Engine Flywheel with Automatic Transmission

1. Install EN-43653 flywheel holding tool (1) in the starter assembly location, engaging the flywheel, in order to prevent crankshaft rotation.
2. Remove the flywheel attaching bolts.
3. Remove the flywheel (1).
4. Remove EN-43653 flywheel holding tool .