For 1990-2009 cars

#### Special Tools

• | EN 47839 Crankshaft Rear Oil Seal Installation Tool

• | EN 42183 Handle

For equivalent regional tools, refer to Special Tools.

1. Place a 3 mm (0.118 in) bead of RTV sealant to the oil pan as shown. Refer to Adhesives, Fluids, Lubricants, and Sealers for the recommended sealant.
2. Place a 3 mm (0.118 in) bead of RTV sealant to the NEW crankshaft rear oil seal housing as shown (1). Refer to Adhesives, Fluids, Lubricants, and Sealers for the recommended sealant.
3. Install the EN 47839 installer with the EN 42183 handle (1, 2) onto the rear of the crankshaft flange.
4. Install the 2 bolts (3).

Note: DO NOT allow any engine oil on the area where the crankshaft rear oil seal housing is to be installed.

5. Install the crankshaft rear oil seal housing (2) to the engine block.
6. Install the 5 crankshaft rear oil seal housing bolts (2).

Caution: Refer to Fastener Caution in the Preface section.

7. Tighten the 5 crankshaft rear oil seal housing bolts in sequence as shown 10 N·m (89 lb in).
8. Tighten the 2 oil pan bolts 10 N·m (89 lb in).
9. Remove the 2 bolts (3).
10. Remove the EN 47839 installer and EN 42183 handle (1, 2) from the crankshaft flange.