For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the engine shield. Refer to Engine Shield Replacement.
3. All Wheel Drive (AWD): Lower the subframe approx. 10 cm. Refer to Frame Replacement.

1 | Transmission Rear Mount Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 100 N·m (74 lb ft)
2 | Transmission Rear Mount Fastener Tighten 62 N·m (46 lb ft)
3 | Transmission Rear Mount Fastener (Qty: 2) Tighten 100 N·m (74 lb ft)
4 | Transmission Rear Mount