For 1990-2009 cars

## Engine Coolant Fan Shroud Replacement Diesel

Callout | Component Name
--- | ---

#### Procedure

Remove the fan shroud. Refer to Engine Coolant Fan Motor Replacement

Tip
To replace the fan shroud see operation Engine Coolant Fan Motor Replacement.

## Engine Coolant Fan Shroud Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the radiator. Refer to Radiator Replacement.

1 | Engine Coolant Fan Motor Fastener (Qty: 3)

#### Procedure

Disconnect the electrical connector of the engine coolant fan motor.

Caution: Refer to Fastener Caution in the Preface section.

Tighten
X N·m (X lb ft)

2 | Engine Coolant Fan Motor
3 | Engine Coolant Fan Motor Fastener (Qty: 3)

#### Procedure

Disconnect the electrical connector of the engine coolant fan motor.

Tighten
X N·m (X lb ft)

4 | Engine Coolant Fan Motor
5 | Engine Coolant Fan Shroud

## Engine Coolant Fan Shroud Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the radiator. Refer to Radiator Replacement.

1 | Engine Coolant Fan Motor Fastener (Qty: 3)

#### Procedure

Disconnect the electrical connector of the engine coolant fan motor.

Caution: Refer to Fastener Caution in the Preface section.

2 | Engine Coolant Fan Motor
3 | Engine Coolant Fan Shroud