For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Place the front door window in the full down position.
2. Remove the front side door window outer sealing strip. Refer to Front Side Door Window Outer Sealing Strip Replacement.

1 | Front Side Door Window Frame Rear Cover Fastener (Qty: 3)

#### Procedure

Pull the front side door window weatherstrip from the applique to expose the fasteners.

2 | Front Side Door Window Frame Rear Cover