For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove engine appearance cover replacement. Refer to XXX.
2. Release the Fuel Feed Pipe. Refer to Fuel Feed Pipe Replacement.
3. Release the Fuel Tank Filler Evaporative Emission Pipe. Refer to LINK.

1 | Engine Appearance Cover Bracket Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Release the electrical cable retainers.

Tighten
X N·m (X lb ft)

2 | Engine Appearance Cover Bracket