For 1990-2009 cars

## Temperature Valve Actuator Replacement - Left Side Left Hand Drive

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel lower trim panel - driver side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
3. Remove the floor air outlet duct - left side. Refer to Floor Air Outlet Duct Replacement - Left Side.

1 | Temperature Valve Actuator Fastener (Qty: 2)

#### Procedure

Disconnect the temperature actuator electrical connector.

2 | Temperature Valve Actuator Tip Actuator is self-calibrating when connecting the battery.