For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Hood Hinge Fastener (Qty: 2)

#### Procedure

1. Loosen the fasteners that secure the hood.
2. Adjust the hood in order to obtain an even gap on both sides between the hood and the fenders and so that the hood is flush with both fenders on the front edge.

2 | Hood Hinge Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Tighten the fasteners in order to secure the hood to the hood hinges.

Tighten
20 N·m (15 lb ft)