For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front wheelhouse rear liner. Refer to Front Wheelhouse Rear Liner Replacement.
2. Disconnect the front side turn signal lamp electrical connector.
3. Squeeze the lamp housing locking retainer and push outward in order to remove the front side turn signal lamp from the fender panel.

1 | Front Side Turn Signal Lamp Tip Replace the bulb, as needed.