For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia in order to access the locking tabs on the front bumper fascia outer insert molding. Refer to Front Bumper Fascia Replacement.

1 | Front Bumper Fascia Outer Insert Molding

#### Procedure

1. Using a small flat-bladed tool, pull and release the outer front bumper fascia locking retainer from the front bumper fascia outer insert molding lower grille.
2. Release the 11 flat locking tabs from the front bumper fascia.
3. Push the front bumper fascia outer insert molding lower grille outward from the front bumper fascia in order to remove.