For 1990-2009 cars

## Intake Manifold Removal 2H0

1. Remove the 2 intake manifold support bolts (2, 3).
2. Remove the intake manifold support (1).
3. Remove the 7 intake manifold bolts (1).
4. Remove the intake manifold.

## Intake Manifold Removal LDE

1. Remove the 2 intake manifold support bolts (2, 3).
2. Remove the intake manifold support (1).
3. Remove the 7 intake manifold bolts (1).
4. Remove the intake manifold.

## Intake Manifold Removal LLU

1. Remove the 5 intake manifold bolts (1).
2. Remove the 3 intake manifold nuts (2).
3. Remove the intake manifold (3) from the cylinder head (5).
4. Remove the intake manifold sealing (4).