For 1990-2009 cars

## Driver or Passenger Seat Adjuster Vertical Actuator Replacement 4-Way Hybrid, 6-Way Hybrid, 6-Way Hyb

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the Driver or Passenger Seat. Refer to Driver or Passenger Seat Replacement.
3. Disconnect the negative battery cable. Refer to Front Bumper Fascia Replacement.
4. Remove Front Seat Adjuster Track Finish Cover. Refer to Front Seat Adjuster Track Finish Cover Replacement.

1 | Seat Adjuster Vertical Actuator Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electric connector.

Tighten
X N·m (X lb in)

2 | Securing Clip
3 | Roll Pin
4 | Seat Adjuster Vertical Actuator