For 1990-2009 cars

## Engine Flywheel Removal 2H0

#### Special Tools

EN-652 Flywheel Holder

For equivalent regional tools, refer to Special Tools.

1. Install the EN-652 holder (1), lock the flywheel via the starter ring gear.
2. Loosen the 6 flywheel bolts.
3. Remove the EN-652 holder (1).
4. Remove the 6 flywheel bolts (1, 2).
5. Remove the flywheel (3).

## Engine Flywheel Removal LLU

#### Special Tools

EN-652 Flywheel Holder

For equivalent regional tools, refer to Special Tools.

1. Install the EN-652 holder (1), lock the flywheel (2) via the starter ring gear.
2. Loosen the 6 flywheel bolts
3. Remove the EN-652 holder (1).
4. Remove the 6 flywheel bolts (2).
5. Remove the flywheel (1).