For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the wiper arm up off the windshield.

1 | Windshield Wiper Blade Cap Tip Use a small flat-bladed tool to open the cap.
2 | Windshield Wiper Blade

#### Procedure

1. Push upward the windshield wiper blade.
2. Slide the windshield wiper blade from the wiper arm.
3. Carefully release the wiper arm back to the windshield.

3 | Windshield Washer Blade Assembly Tip Discard if rubber appears worn or does not wipe the windshield clean.