For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheelhouse front liner. Refer to Front Wheelhouse Front Liner Replacement.
3. Disconnect fog lamp bulb socket electrical connector.

1 | Front Fog Lamp (Qty: 2)
2 | Front Fog Lamp Retainer Tip Use a small flat-bladed tool to release the retainer from the front bumper fascia.
3 | Front Fog Lamp Warning: Halogen bulbs contain gas under pressure. Handling a bulb improperly could cause it to shatter into flying glass fragments. To help avoid personal injury:

• | Turn off the lamp switch and allow the bulb to cool before changing the bulb.

• | Leave the lamp switch OFF until the bulb change is complete.

• | Always wear eye protection when changing a halogen bulb.

• | Handle the bulb only by its base. Avoid touching the glass.

• | Keep dirt and moisture off the bulb.

• | Properly dispose of the used bulb.

• | Keep halogen bulbs out of the reach of children.

#### Procedure

Remove the lamp from the fog lamp bracket.